**Template 4.19 D**

**Vehicle Recovery Kit**

* Two 4,750kg bow shackles
* One 8,000kg (Min. breaking strength) snatch strap
* One pair of gloves
* One carry bag

**Template 4.19 E**

**Winch Recovery Accessories**

* One 8,000kg snatch strap
* One 12,000kg tree trunk protector
* One 4,500kg winch extension strap
* One snatch block
* Two 4,750kg bow shackles (19mm, 3/4inch)
* A pair of leather gloves
* One recovery damper



**Template 4.19 F**

**Manual Recovery Package**

* Hand winch
* Front and rear recovery points (Subject to vehicle applicability)
* Winch recovery accessories bag containing: One 8,000kg recovery strap, two 4,750kg bow shackles, one recovery strap extension, one tree trunk protector, one snatch block, one cable damper and a pair of leather gloves
* Sand mats (sand ladders)
* Folding shovel



**Template 4.19 G**

**Hand Winch**

* Made from high quality steel and aluminium components
* Pulling capacity - 2,400kg
* Rated lifting Capacity - 1,600kg
* Dimensions - 545x280x97mm
* Stainless steel 20m cable
* Cable diameter - 11mm
* Handle length closed - 800mm
* Handle length extended - 1,200mm
* Heavy duty canvas bag



**Template 4.19 H**

**Electric Winch**

* Rated line pull: 4,536 kg (10,000lbs) single-line
* 12V series wound motor
* Remote control with wireless capability
* 3-Stage planetary gear train
* Gear ratio: 218:1
* Clutch (free-spooling)
* Synthetic rope: 27.4m, 9.5mm diam. (90 ft, 3/8 in dia.)
* Fairlead: Cast iron hawse
* Powder-coat finish

